**OBRAZAC ZA IZRADU KOMERCIJALNE PONUDE – Laboratorijsko staklo, potrošni materijal, pomoćni pribor i rezervni dijelovi**

**PONUĐAČ: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**Ponuda broj: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **R. br.** | **Naziv** | **Tip/ Proizvođač** | **Planirana količina** | **Napomena** | | **Jed. Cijena u \_\_ bez PDV-a** | **Ukupno u \_\_ bez PDV-a** |
| 1. | Laboratorijske čaše-bez izljeva | 400 ml, VF | 10 kom. | Klasa A | |  |  |
| 2. | Menzura VF bez izljevom,  klasa A | 1000 ml, (plava) | 6 kom. | AD0892-C00, Scavin | |  |  |
| 3. | Filter papir od staklenih vlakana-EN12662:   * Prečnik 47 mm; * Pore size 0,70 µm; * 1/100 kom.; | FiltrTECH | 3 pak. | FV25A0047 | |  |  |
| 4. | Membrane filter (Cellulose mixed ester - MCE),  - pore size 0,8 µm:  - prečnik 47 mm;  - 1/100 kom.; | LabExpert | 4 pak. | PF000212 | |  |  |
| 5. | Membrane filter (Cellulose Nitrate Filter),  - pore size 0,8 µm:  - prečnik 47 mm;  - 1/100 kom.; | Sartorius | 3 pak. | 11404-47-ACN | |  |  |
| 6. | NYLON MEMBRANES 0,80 µm:   * Diam.: 47 mm; * Pore size 0,80 µm; * Qty.: 100 kom.; | FiltrTECH | 1 pak. | Ref.:MF047NY080 | |  |  |
| 7. | Šprica, plastična, 2ml | 2 ml | 500 kom. |  | |  |  |
| 8. | Igle |  | 400 kom. |  | |  |  |
| 9. | Digital alarm timer „Count Down-Up“:  - Big 6-digit LCD  - Digital stopwatch (counting up)  - Short timer (counting down)  - With memory function  - Stopwatch and countdown up to 23 h 59 min. 59 sec.  - Optical and acoustic alarm when a timer expires  - Incl. magnet for mounting, hanging bracket and stand (fold-out | LLG | 4 kom. | Part No.:6311351\*LLG | |  |  |
| 10. | Luer Slip Tip Šprice od 3 mL sa elastomernim vrhom, nesterilne, 1/100 kom; | BD | 5 pak. | P/N P23438 | |  |  |
| 11. | Šprice (Injekt Luer Solo) od 10 mL sa elastomernim vrhom, nesterilne, 1/100 kom; | B/BRAUN | 5 pak. | Ref. 4606108V | |  |  |
| 12. | Mrežice željezne zaštitne 120X120 mm | J.P. Selecta | 5 kom. | 1087122 | |  |  |
| 13. | Mrežice željezne zaštitne 160X160 mm | J.P. Selecta | 5 kom. | 1087162 | |  |  |
| 14. | Lončić porculanski za žarenje, 1/45 DIN, low | KEFO | 10 kom. | 9250906\*LLG | |  |  |
| 15. | Laboratory mats, silicone (Black)  350x350 mm | KEFO | 4 kom. | 9.390 093 | |  |  |
| 16. | Spatulas with a wooden handle, stainless steel; 20x130x230mm | LLG | 2 kom. | 9220613\*LLG | |  |  |
| 17. | Digitron, CITIZEN SR-260N | CITIZEN | 5 kom. |  | |  |  |
| 18. | Petri dish with cover, stakleni  (e.g. 80mmx15mm) | - | 5 kom. |  | |  |  |
| 19. | Hydrocarbon Mix, C12/C14/C16 | Shimadzu | 2 kom. | 44072-U | |  |  |
| 20. | Gamma-BHC, 1y1ml, Hexane, 0.1 ug/mL; GC 2030 | Shimadzu | 2 kom. | 44088U | |  |  |
| 21. | Pipeta (za viskozna maziva) | Gilson, M1000E | 2 kom. |  | |  |  |
| 22. | Nastavci (za viskozna maziva) | Gilson, CP1000; Pak od 960 kom. | 1 pak. |  | |  |  |
| 23. | Pyrex glass jar | Scavini, Italija | 1 kom. | AD0892-S09 | |  |  |
| 24. | Vacuum Pump, Rocker 300 | ROCKER | 1 kom. | Šifra: 167300-11 (22), AC220V/50Hz | |  |  |
| 25. | Filtration Apparatus VF7 | ROCKER | 1 kom. | Model VF7  Cat. No. 167200-07  ▸ Flask capacity: 1000 mL; ▸ Filter diameter: 47 mm; | |  |  |
| 26. | Funnel 300 mL, borosilicate glass for VF3/6/7 | ROCKER | 2 kom. | 00829 167210-03 | |  |  |
| 27. | Upaljač za COC-CLA 5 AP/  Elektric Ignitet | Anton Paar | 1 kom. | Cat. No. 107206 | |  |  |
| 28. | Synthetic wadding for Fresenius column, pack of 250 g | 7320 Linetronic | 5 kom. | Za NOACK test LINETRONIC | |  |  |
| 29. | Termometar – Tip ASTM 19C | SLW ili AMA | 4 kom. | Punjen Hg! | |  |  |
| 30. | Termometar – Tip ASTM 21C | SLW ili AMA | 4 kom. | Punjen Hg! | |  |  |
| 31. | Test Tube ASTM D130, Pack of 10 pcs | 2093  Linetronic | 2 kom. | • Made in glass,  • 25 mm diameter × 150 mm height., | |  |  |
| 32. | Copper Corrosion Test Vessel | 5597  Linetronic | 2 kom. | * Stainless steel, * 10 bar pressur certificate, * For liquid model only. | |  |  |
| 33. | Test Specimen, ASTM D665 A&B | 11220-001 | 5 kom. | STANHOPHE-SETA | |  |  |
| 34. | Test Piece Holder PTFE | 11290-000 | 5 kom. | STANHOPHE-SETA | |  |  |
| 35. | Mott Diffuzer | 14023-0 | 4 kom. | STANHOPHE-SETA | |  |  |
| 36. | Rubber stoppers pack of 2 pcs | LAB-101-882  Linetronic | 2 pak. |  | |  |  |
| 37. | Air-inlet tube | LAB-101-915/T  Linetronic | 4 kom. |  | |  |  |
| 38. | Silicon Carbide Paper, 100 grit;  ASTM D 130 | Linetronic | 100 pcs. | • 7146 | |  |  |
| 39. | Silicon Carbide Paper, 240 grit;  ASTM D 130 | Linetronic | 100 psc. | • 7060 | |  |  |
| 40. | Silicon Carbide Grains, 150 mesh; ASTM D 130 | Linetronic | 1 kg | • 7062 | |  |  |
| 41. | Silicon Oil for Liquid Bath,  ASTM D130 & ASTM D6082 | Tamson  200-50 | 2x20L | • silicone oil, kinematic viscosity 9,0 mm²/s at 150°C, | |  |  |
| 42. | Apparatus for test maximum diameter/permeability of diffusers, ASTM D892 | Linetronic/Scavini | 1 set | • 5232:. Air compressor with filter.  . Air regulator and U-tube manometer.  . Glass calibrated cylinder with delivery tube.  . Filtering flask wide mouth with rubber stopper and delivery tube.  . Digital flowmeter 1.2 to 60 nL/min with calibration certificate.  • LAB-892-099: VL Reference liquid.  . Bottle of 1.0 liter approx.  . 1 year shelf life.  . Foam value acc. ASTM D892. | |  |  |
| 43. | Bireta automatska po Pelletu od 10 mL; Tamna | Witeg | 2 kom. |  | |  |  |
| 44. | Baterija 3,6V; Li-SOCl2 | LSAFT  LS 14250 | 20 kom. |  | |  |  |
| 45. | Digital Refractometer ORM 1CA | KERN | 2 kom. |  | |  |  |
| 46. | Digital Refractometer ORM 2CA | KERN | 2 kom. |  | |  |  |
| 47. | Generatorska elektroda sa dijafrgmom | 60.344.100, Methrom | 1 kom. |  | |  |  |
| 48. | Kulometrijska ćelija-čaša  (80-250 ml) za KF | 61.464.320,  Metrohm | 1 kom. |  | |  |  |
| 49. | Dupla platinska elektroda za KF | 60.341.100,  Metrohm | 1 kom. |  | |  |  |
| 50. | Septum 16mm, 5 kom. | Metrohm 61.448.020 | 2 set. |  | |  |  |
| 51. | KF adsorber cijev za kulometrijsku čašu | Metrohm 61.403.030 | 1 kom. |  | |  |  |
| 52. | SGJ stopper SGJ 14  (čep za titracijsku čašu) | Metrohm 61.403.000 | 1 kom. |  | |  |  |
| 53. | Čep sa otvorom za septem | Metrohm 62.701.040 | 1 kom. |  | |  |  |
| 54. | Aquastar® CombiCoulomat frit | Metrohm 1.092.550.500 | 1 kom. |  | |  |  |
| 55. | Viskozimetri UBBELOHDE  (ASTM D 445-ASTM D 446-ISO 3104-ISO 3105), V= 18mL | Size: 1 | 2 kom. | Nominalna konstanta C=0,01  Sertifikat o kalibraciji obavezan. | |  |  |
| 56. | Viskozimetri UBBELOHDE  (ASTM D 445-ASTM D 446-ISO 3104-ISO 3105), V= 18mL | Size: 1C | 2 kom. | Nominalna konstanta C=0,03  Sertifikat o kalibraciji obavezan. | |  |  |
| 57. | Viskozimetri UBBELOHDE  (ASTM D 445-ASTM D 446-ISO 3104-ISO 3105), V= 18mL | Size: 1B | 2 kom. | Nominalna konstanta C=0,05  Sertifikat o kalibraciji obavezan. | |  |  |
| 58. | Viskozimetri UBBELOHDE  (ASTM D 445-ASTM D 446-ISO 3104-ISO 3105), V= 18mL | Size: 2 | 2 kom. | Nominalna konstanta C=0,1  Sertifikat o kalibraciji obavezan. | |  |  |
| 59. | Viskozimetri UBBELOHDE  (ASTM D 445-ASTM D 446-ISO 3104-ISO 3105), V= 18mL | Size: 3 | 2 kom. | Nominalna konstanta C=1,0  Sertifikat o kalibraciji obavezan. | |  |  |
| 60. | Viskozimetri UBBELOHDE  (ASTM D 445-ASTM D 446-ISO 3104-ISO 3105), V= 18mL | Size: 3C | 2 kom. | Nominalna konstanta C=3,0  Sertifikat o kalibraciji obavezan. | |  |  |
| 61. | O-Ring for sample container | Scavini,  SN:1025169 | 1 pak. | OR3143 | |  |  |
| 62. | Seeding container, AD1177-C01 | Scavini,  SN:1025169 | 5 kom. |  | |  |  |
| 63. | Glass sample container, AD1177-C10 | Scavini,  SN:1025169 | 5 kom. |  | |  |  |
| 64. | Detektor Focus 5+ za XRF | Oxford  Kat. Br. 45693 | 1 kom. |  | |  |  |
| 65. | Amortizeri za XRF (TwinX) | Oxford  GS-12-40-BB-180 | 2 kom. |  | |  |  |
| 66. | Kopča poklopca na TwinX-u | - | 1 kom. |  | |  |  |
| 67. | Fini prah za D1384/Silicijum-karbid | - | 2 kg | Granulacija:  F220  (53-75µm) | |  |  |
| 68. | Četka od čekinje (prirodna)   * Φ četke D1: 5mm | LESSMANN®  Art. Br. 5749495 | 10 kom. |  | |  |  |
| 69. | Četka od mesinga:   * ukupna dužina 225 mm, * dužina korišćenja 90 mm, * žica - fi:0,25 mm, | BERNER  Ar. Nr175780 | 5 kom. | Ručna žičana mesingana četka sa dva reda. | |  |  |
| NAČIN PLAĆANJA | | | | |  | | |
| ROK ISPORUKE | | | | |  | | |
| MJESTO ISPORUKE | | | | |  | | |
| GARANTNI ROK | | | | |  | | |
| ROK VAŽENJA PONUDE | | | | |  | | |

Datum: \_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Potpis i pečat Ponuđača